Please install the driver if the instrument or communication is not normal for the first time

Installation method of USB drive:

Recommended method 1

1. Use the driver ftdi_ft232_drive.exe, double-click to install, then plug in the device and it will be recognized automatically.Windows 7 64-bit or above, please run in administrator mode.

2. Use the inf file installation method, suitable for users with invalid method 1.
A) plug in the device, perform the search driver installation wizard, and select the directory as the folder where the inf driver is located.
B) two consecutive installations